[preset00]
fRating=2.000000
fGammaAdj=1.000000
fDecay=1.000000
fVideoEchoZoom=5.427025
fVideoEchoAlpha=0.500000
nVideoEchoOrientation=3
nWaveMode=6
bAdditiveWaves=0
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=0
bMaximizeWaveColor=1
bTexWrap=1
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=100.000000
fWaveScale=0.972360
fWaveSmoothing=0.500000
fWaveParam=1.000000
fModWaveAlphaStart=0.500000
fModWaveAlphaEnd=1.000000
fWarpAnimSpeed=0.010000
fWarpScale=1.766487
fZoomExponent=1.000000
fShader=0.000000
zoom=1.000000
rot=0.000000
cx=0.500000
cy=0.500000
dx=0.000010
dy=0.000010
warp=0.010000
sx=1.000000
sy=1.000000
wave_r=0.000000
wave_g=0.000000
wave_b=0.000000
wave_x=0.400000
wave_y=0.500000
ob_size=0.000000
ob_r=0.000000
ob_g=0.000000
ob_b=0.000000
ob_a=1.000000
ib_size=0.000000
ib_r=0.000000
ib_g=0.000000
ib_b=0.000000
ib_a=0.000000
nMotionVectorsX=6.400000
nMotionVectorsY=4.800000
mv_dx=0.000000
mv_dy=0.000000
mv_l=5.000000
mv_r=1.000000
mv_g=1.000000
mv_b=1.000000
mv_a=0.000000
per_frame_1=wave_r = wave_r + 0.35*sin(1.4*time) + 0.15*sin(2.5*time+2*mid);
per_frame_2=wave_g = wave_g + 0.35*sin(1.7*time) + 0.15*sin(2.11*time+2.2*treb);
per_frame_3=wave_b = wave_b + 0.35*sin(1.84*time) + 0.15*sin(2.3*time+2*bass);
per_frame_4=//wave_y = wave_y + 0.24*sin(2.5*time);
per_frame_5=wave_x = 0.75 + 0.45*sin(sin(0.5*bass_att-0.4*treb_att)*sin(time));
per_frame_6=//warp = warp + (0.8*bass_att - 0.8*treb_att)*0.25;
per_pixel_1=//thresh = above(bass_att,thresh)*2+(1-above(bass_att,thresh))*((thresh-1.3)*0.96+1.3);
per_pixel_2=//dx_r = equal(thresh,2)*0.015*sin(5*time)+(1-equal(thresh,2))*dx_r;
per_pixel_3=//dy_r = equal(thresh,2)*0.015*sin(6*time)+(1-equal(thresh,2))*dy_r;
per_pixel_4=
per_pixel_5=//warp = warp + dy_r*50* (if (above(x*cos(1.2*time), sin(1.62*time)), if(below(x*sin(1.72*time),cos(1.8*time)), if(below(y,sin(3*time)), + 1*bass, 0), 0), 0));
per_pixel_6=
per_pixel_7=dy = dy + (0.004*sin(cos(x*2.25*time)*0.86*sin(0.52*time*cos(max(0.075*bass_att,0.0005*time)))));
per_pixel_8=dx = dx + (0.004*cos(sin(y*2.25*time)*0.94*sin(0.79*time*sin(max(0.075*treb_att,0.0005*time)))));
per_pixel_9=dy = dy - sin((1+x)*time*0.94)*(0.005*above(y,sin(1.14*time+0.02*treb_att)));
per_pixel_10=dx = dx + sin((0.25-y)*time*0.97)*(0.005*above(x,cos(1.2*time+0.02*bass_att)));
